[37mNothing to do, check usage "gpac -h"
gpac - GPAC command line filter engine - version 2.5-DEV-rev1517-g120c6944f-buildbot-route-repair
(c) 2000-2024 Telecom Paris distributed under LGPL v2.1+ - https://gpac.io

Please cite our work in your research:
	GPAC Filters: https://doi.org/10.1145/3339825.3394929
	GPAC: https://doi.org/10.1145/1291233.1291452

[0msession error: Bad Parameter
[33mNo filter chain found for PID A2 in filter mp4dmx to any loaded filters - Will try to remove
[0mx265 [info]: HEVC encoder version 4.1+1-1d117be
x265 [info]: build info [Mac OS X][clang 16.0.0][64 bit] 10bit
x265 [info]: using cpu capabilities: NEON Neon_DotProd Neon_I8MM
x265 [warning]: lowering VBV buffer size to 40000Kb
x265 [info]: Main 10 profile, Level-5.1 (Main tier)
x265 [info]: Thread pool created using 8 threads
x265 [info]: Slices                              : 1
x265 [info]: frame threads / pool features       : 3 / wpp(34 rows)
x265 [info]: Coding QT: max CU size, min CU size : 64 / 8
x265 [info]: Residual QT: max TU size, max depth : 32 / 1 inter / 1 intra
x265 [info]: ME / range / subpel / merge         : hex / 57 / 2 / 3
x265 [info]: Lookahead / bframes / badapt        : 20 / 2 / 0
x265 [info]: b-pyramid / weightp / weightb       : 1 / 1 / 0
x265 [info]: References / ref-limit  cu / depth  : 3 / off / on
x265 [info]: AQ: mode / str / qg-size / cu-tree  : 2 / 1.0 / 32 / 1
x265 [info]: Rate Control / qCompress            : ABR-17000 kbps / 0.60
x265 [info]: VBV/HRD buffer / max-rate / init    : 40000 / 25500 / 0.900
x265 [info]: tools: rd=3 psy-rd=2.00 early-skip rskip mode=1 signhide tmvp
x265 [info]: tools: b-intra strong-intra-smoothing lslices=8 deblock sao
x265 [info]: tools: dhdr10-info
x265 [info]: frame I:      6, Avg QP:27.69  kb/s: 58096.13
x265 [info]: frame P:    167, Avg QP:29.21  kb/s: 29721.57
x265 [info]: frame B:    327, Avg QP:34.13  kb/s: 7839.47 
x265 [info]: Weighted P-Frames: Y:0.0% UV:0.0%

encoded 500 frames in 255.16s (1.96 fps), 15751.17 kb/s, Avg QP:32.41


================================================================

/usr/local/bin/gpac -i "/Users/ndvx/code/cta_wave/mezzanine/5/splice_main_sol_sdr_bt2020_C1_3840x2160@50_10.mp4":#StartNumber=-2000000:#Representation=1:#IsoBrand=cud1:FID=GEN2_splice_main  ffsws:osize=3840x2160:ofmt=yuv420_10:SID=GEN2_splice_main @ enc:gfloc:c=libx265:b=17000k:bf=2:fintra=48/25:g=96:profile=main10:color_primaries=9:color_trc=14:colorspace=9::x265-params="scenecut=0:no-open-gop=1:b-adapt=0:level-idc=51:no-high-tier=1:vbv-bufsize=51000:vbv-maxrate=25500:sar=1\:1"::FID=V0 --bs_switch=off  -o batch/cud1_sets/12.5_25_50/splice_main/2025-06-30/stream.mpd:profile=live:ctmode=negctts:cmaf=cmf2:segdur=48/25:tpl:template=\$Init=1/init\$\$Segment=1/\$:stl:cdur=48/25:SID=V0

================================================================



================================================================

